---
id: record
title: Recording
---

import ConfigTabs from "@site/src/components/ConfigTabs";
import TabItem from "@theme/TabItem";
import NavPath from "@site/src/components/NavPath";

Recordings can be enabled and are stored at `/media/frigate/recordings`. The folder structure for the recordings is `YYYY-MM-DD/HH/<camera_name>/MM.SS.mp4` in **UTC time**. These recordings are written directly from your camera stream without re-encoding. Each camera supports a configurable retention policy. Frigate chooses the largest matching retention value between the recording retention and the tracked object retention when determining if a recording should be removed.

New recording segments are written from the camera stream to cache, they are only moved to disk if they match the setup recording retention policy.

H265 recordings can be viewed in Chrome 108+, Edge and Safari only. All other browsers require recordings to be encoded with H264.

## Common recording configurations

### Most conservative: Ensure all video is saved

For users deploying Frigate in environments where it is important to have contiguous video stored even if there was no detectable motion, the following configuration will store all video for 3 days. After 3 days, only video containing motion will be saved for 7 days. After 7 days, only video containing motion and overlapping with alerts or detections will be retained until 30 days have passed.

<ConfigTabs>
<TabItem value="ui">

Navigate to <NavPath path="Settings > Global configuration > Recording" />.

- Set **Enable recording** to on
- Set **Continuous retention > Retention days** to `3`
- Set **Motion retention > Retention days** to `7`
- Set **Alert retention > Event retention > Retention days** to `30`
- Set **Alert retention > Event retention > Retention mode** to `all`
- Set **Detection retention > Event retention > Retention days** to `30`
- Set **Detection retention > Event retention > Retention mode** to `all`

</TabItem>
<TabItem value="yaml">

```yaml
record:
  enabled: True
  continuous:
    days: 3
  motion:
    days: 7
  alerts:
    retain:
      days: 30
      mode: all
  detections:
    retain:
      days: 30
      mode: all
```

</TabItem>
</ConfigTabs>

### Reduced storage: Only saving video when motion is detected

To reduce storage requirements, configure recording to only retain video where motion or activity was detected.

<ConfigTabs>
<TabItem value="ui">

Navigate to <NavPath path="Settings > Global configuration > Recording" />.

- Set **Enable recording** to on
- Set **Motion retention > Retention days** to `3`
- Set **Alert retention > Event retention > Retention days** to `30`
- Set **Alert retention > Event retention > Retention mode** to `motion`
- Set **Detection retention > Event retention > Retention days** to `30`
- Set **Detection retention > Event retention > Retention mode** to `motion`

</TabItem>
<TabItem value="yaml">

```yaml
record:
  enabled: True
  motion:
    days: 3
  alerts:
    retain:
      days: 30
      mode: motion
  detections:
    retain:
      days: 30
      mode: motion
```

</TabItem>
</ConfigTabs>

### Minimum: Alerts only

If you only want to retain video that occurs during activity caused by tracked object(s), this configuration will discard video unless an alert is ongoing.

<ConfigTabs>
<TabItem value="ui">

Navigate to <NavPath path="Settings > Global configuration > Recording" />.

- Set **Enable recording** to on
- Set **Continuous retention > Retention days** to `0`
- Set **Alert retention > Event retention > Retention days** to `30`
- Set **Alert retention > Event retention > Retention mode** to `motion`

</TabItem>
<TabItem value="yaml">

```yaml
record:
  enabled: True
  continuous:
    days: 0
  alerts:
    retain:
      days: 30
      mode: motion
```

</TabItem>
</ConfigTabs>

## Pre-capture and Post-capture

The `pre_capture` and `post_capture` settings control how many seconds of video are included before and after an alert or detection. These can be configured independently for alerts and detections, and can be set globally or overridden per camera.

<ConfigTabs>
<TabItem value="ui">

Navigate to <NavPath path="Settings > Global configuration > Recording" /> for global defaults, or <NavPath path="Settings > Camera configuration > (select camera) > Recording" /> to override for a specific camera.

| Field                                          | Description                                          |
| ---------------------------------------------- | ---------------------------------------------------- |
| **Alert retention > Pre-capture seconds**      | Seconds of video to include before an alert event    |
| **Alert retention > Post-capture seconds**     | Seconds of video to include after an alert event     |
| **Detection retention > Pre-capture seconds**  | Seconds of video to include before a detection event |
| **Detection retention > Post-capture seconds** | Seconds of video to include after a detection event  |

</TabItem>
<TabItem value="yaml">

```yaml
record:
  enabled: True
  alerts:
    pre_capture: 5 # seconds before the alert to include
    post_capture: 5 # seconds after the alert to include
  detections:
    pre_capture: 5 # seconds before the detection to include
    post_capture: 5 # seconds after the detection to include
```

</TabItem>
</ConfigTabs>

- **Default**: 5 seconds for both pre and post capture.
- **Pre-capture maximum**: 60 seconds.
- These settings apply per review category (alerts and detections), not per object type.

### How pre/post capture interacts with retention mode

The `pre_capture` and `post_capture` values define the **time window** around a review item, but only recording segments that also match the configured **retention mode** are actually kept on disk.

- **`mode: all`** — Retains every segment within the capture window, regardless of whether motion was detected.
- **`mode: motion`** (default) — Only retains segments within the capture window that contain motion. This includes segments with active tracked objects, since object motion implies motion. Segments without any motion are discarded even if they fall within the pre/post capture range.
- **`mode: active_objects`** — Only retains segments within the capture window where tracked objects were actively moving. Segments with general motion but no active objects are discarded.

This means that with the default `motion` mode, you may see less footage than the configured pre/post capture duration if parts of the capture window had no motion.

To guarantee the full pre/post capture duration is always retained:

```yaml
record:
  enabled: True
  alerts:
    pre_capture: 10
    post_capture: 10
    retain:
      days: 30
      mode: all # retains all segments within the capture window
```

:::note

Because recording segments are written in 10 second chunks, pre-capture timing depends on segment boundaries. The actual pre-capture footage may be slightly shorter or longer than the exact configured value.

:::

### Where to view pre/post capture footage

Pre and post capture footage is included in the **recording timeline**, visible in the History view. Note that pre/post capture settings only affect which recording segments are **retained on disk** — they do not change the start and end points shown in the UI. The History view will still center on the review item's actual time range, but you can scrub backward and forward through the retained pre/post capture footage on the timeline. The Explore view shows object-specific clips that are trimmed to when the tracked object was actually visible, so pre/post capture time will not be reflected there.

## Will Frigate delete old recordings if my storage runs out?

As of Frigate 0.12 if there is less than an hour left of storage, the oldest 2 hours of recordings will be deleted.

## Configuring Recording Retention

Frigate supports both continuous and tracked object based recordings with separate retention modes and retention periods.

:::tip

Retention configs support decimals meaning they can be configured to retain `0.5` days, for example.

:::

### Continuous and Motion Recording

The number of days to retain continuous and motion recordings can be configured. By default, continuous recording is disabled.

<ConfigTabs>
<TabItem value="ui">

Navigate to <NavPath path="Settings > Global configuration > Recording" />.

| Field                                     | Description                                  |
| ----------------------------------------- | -------------------------------------------- |
| **Enable recording**                      | Enable or disable recording for all cameras  |
| **Continuous retention > Retention days** | Number of days to keep continuous recordings |
| **Motion retention > Retention days**     | Number of days to keep motion recordings     |

</TabItem>
<TabItem value="yaml">

```yaml
record:
  enabled: True
  continuous:
    days: 1 # <- number of days to keep continuous recordings
  motion:
    days: 2 # <- number of days to keep motion recordings
```

</TabItem>
</ConfigTabs>

Continuous recording supports different retention modes [which are described below](#configuring-recording-retention).

### Object Recording

The number of days to retain recordings for review items can be specified for items classified as alerts as well as tracked objects.

<ConfigTabs>
<TabItem value="ui">

Navigate to <NavPath path="Settings > Global configuration > Recording" />.

| Field                                                      | Description                                 |
| ---------------------------------------------------------- | ------------------------------------------- |
| **Enable recording**                                       | Enable or disable recording for all cameras |
| **Alert retention > Event retention > Retention days**     | Number of days to keep alert recordings     |
| **Detection retention > Event retention > Retention days** | Number of days to keep detection recordings |

</TabItem>
<TabItem value="yaml">

```yaml
record:
  enabled: True
  alerts:
    retain:
      days: 10 # <- number of days to keep alert recordings
  detections:
    retain:
      days: 10 # <- number of days to keep detections recordings
```

</TabItem>
</ConfigTabs>

This configuration will retain recording segments that overlap with alerts and detections for 10 days. Because multiple tracked objects can reference the same recording segments, this avoids storing duplicate footage for overlapping tracked objects and reduces overall storage needs.

## Can I have "continuous" recordings, but only at certain times?

Using Frigate UI, Home Assistant, or MQTT, cameras can be automated to only record in certain situations or at certain times.

## How do I export recordings?

Footage can be exported from Frigate by right-clicking (desktop) or long pressing (mobile) on a review item in the Review pane or by clicking the Export button in the History view. Exported footage is then organized and searchable through the Export view, accessible from the main navigation bar.

### Time-lapse export

Time lapse exporting is available only via the [HTTP API](../integrations/api/export-recording-export-camera-name-start-start-time-end-end-time-post.api.mdx).

When exporting a time-lapse the default speed-up is 25x with 30 FPS. This means that every 25 seconds of (real-time) recording is condensed into 1 second of time-lapse video (always without audio) with a smoothness of 30 FPS.

To configure the speed-up factor, the frame rate and further custom settings, use the `timelapse_args` parameter. The below configuration example would change the time-lapse speed to 60x (for fitting 1 hour of recording into 1 minute of time-lapse) with 25 FPS:

```yaml {3-4}
record:
  enabled: True
  export:
    timelapse_args: "-vf setpts=PTS/60 -r 25"
```

:::tip

When using `hwaccel_args`, hardware encoding is used for timelapse generation. This setting can be overridden for a specific camera (e.g., when camera resolution exceeds hardware encoder limits); set the camera-level export hwaccel_args with the appropriate settings. Using an unrecognized value or empty string will fall back to software encoding (libx264).

:::

:::tip

The encoder determines its own behavior so the resulting file size may be undesirably large.
To reduce the output file size the ffmpeg parameter `-qp n` can be utilized (where `n` stands for the value of the quantisation parameter). The value can be adjusted to get an acceptable tradeoff between quality and file size for the given scenario.

:::

## Apple Compatibility with H.265 Streams

Apple devices running the Safari browser may fail to playback h.265 recordings. The [apple compatibility option](../configuration/camera_specific.md#h265-cameras-via-safari) should be used to ensure seamless playback on Apple devices.

## Syncing Media Files With Disk

Media files (event snapshots, event thumbnails, review thumbnails, previews, exports, and recordings) can become orphaned when database entries are deleted but the corresponding files remain on disk.

Normal operation may leave small numbers of orphaned files until Frigate's scheduled cleanup, but crashes, configuration changes, or upgrades may cause more orphaned files that Frigate does not clean up. This feature checks the file system for media files and removes any that are not referenced in the database.

The Maintenance pane in the Frigate UI or an API endpoint `POST /api/media/sync` can be used to trigger a media sync. When using the API, a job ID is returned and the operation continues on the server. Status can be checked with the `/api/media/sync/status/{job_id}` endpoint.

Setting `verbose: true` writes a detailed report of every orphaned file and database entry to `/config/media_sync/<job_id>.txt`. For recordings, the report separates orphaned database entries (DB records whose files are missing from disk) from orphaned files (files on disk with no corresponding database record).

:::warning

This operation uses considerable CPU resources and includes a safety threshold that aborts if more than 50% of files would be deleted. Only run when necessary. If you set `force: true` the safety threshold will be bypassed; do not use `force` unless you are certain the deletions are intended.

:::
